Design of the UV Exposure Box

# Introduction

Basic Operation: The artist will put the image in the box, set the exposure parameters via Web Interface over WiFi, and the start the process. The internal processor will initiate the turning on of the UV LED lighting..

Text, whiteboard

Description automatically generated

The major components, from left to right:

1. LED Control Layer. Proposed name: **UVEB\_LEDControl**. This will entail turning on/off. If I can put in current sensing, it will include that as well.
2. UV Light Sensing Layer, **UVEB\_UVStats**. Measurement of light data captured.
3. UI Control. **UVEB\_UIControl**. There will be some LED status, but principal UI will be HTTP over WiFi. UI will encompass Alarms, Status, Start/Stop commands.
4. Fan Control handling. **UVEB\_FanControl**. Fan on/off. May use PWM to handle fan speed.
5. Temperature Sensing Layer. **UVEB\_TempStatus**. Discovery of 1-wire temp sensors, reading temp data.
6. System Diag handling. **UVEB\_SystemStats**. Aggregate data collection, for use by alarms and events.

# Basic System Architecture:

## LED Control System

The hardware components consist of the following:

1. A LED power circuit with a constant current LED driver.
2. A GPIO to MOSFET switch. The CPU (ESP32) will drive the switch from a GPIO based upon the control algorithm.

The software components:

1. The LED Control Layer (UVEB\_LEDControl).

Basic operation of the UV LEDs. They will turn on when the artist will command the system to go on after the parameters are set. The UV LEDs will turn off either when the artist’s parameters sensed are completed OR if there is an error detected.

## UV Light Sensing System

The hardware components consist of:

1. UV Light sensor(s) that uses a ML8511 (detects 280-390nm light) and can interface with the ESP32 easily.
2. Cables and placement at the bottom of the exposure floor in the box.

The software with consist of interfacing the ESP32 with the suitable device library and will sample the UV data collected at periodic intervals. When the SW determines that the exposure parameters have been met as per artist selection, the SW will issue a System Event to be processed by the Control SW. If the SW determines that the device is not working (sampling) correctly, another System Event will be issued that indicates a system error.